**FILTERS / INDICATORS 🡺 where to find the matching information**

LIFESPAN OF INFRASTRUCTURE 🡺 from QUALITATIVE CRITERIA in criteria 1 (trustworthiness & durability / estimated lifespan for medical use)

BASIC shelter (3 mths < x < 6 mths)

TRANSITIONAL shelter (x < 18 mths)

WAREHOUSE structure (x < 2y)

PREFABRICATED structures (x < 5y)

SIZE OF INFRASTRUCTURE 🡺 from TECHNICAL CRITERIA criteria 2 (physical characteristics / covered surface)

FAMILY size (10m2 < x < 20m2)

POLYVALENT size (20m2 < x < 50m2)

MEDIUM size (50m2 < x < 150m2)

LARGE size (150m2 < x)

THERMAL VALUE 🡺 from QUALITATIVE CRITERIA in criteria 3 (building envelope / thermal performance)

LOW

MEDIUM

HIGH

COST EFFECTIVENESS 🡺 from TECHNICAL CRITERIA criteria 4 (transport & pricing / Price)

LOW (0 < x < 100 €/m²)

MEDIUM (100€/m² < x < 500 €/m²)

HIGH (500 €/m² < x < 1000 €/m²)

Set-up time 🡺 from TECHNICAL CRITERIA criteria 3 (installation / estimated set-up time)

LOW (0 < x < 5h)

MEDIUM (5h < x 2 days)

HIGH (2 days < x)

SPECIFIC FEATURES

- Flooring provided or not 🡺 from TECHNICAL CRITERIA criteria 2 (physical characteristics / floor surface)

- Type of transport : plane, container truck, pickup 🡺 from TECHNICAL CRITERIA criteria 4 (transport & pricing / type of transport)